For 1990-2009 cars

### Removal Procedure

1. Open rear door.
2. Unsnap weatherstrip around rear of roof rail and partially remove.
3. Partially remove weatherstrip in rear door opening.
4. Remove C-pillar applique screws in door opening.
5. Remove C-pillar applique by prying up from the door opening area and then rearward to detach from adhesive strips.
6. Clean old adhesive strips from C-pillar and applique.

### Installation Procedure

1. Install new adhesive strips to C-pillar.
2. Install applique to C-pillar by aligning applique to rear of body.
3. Install applique to C-pillar and install screws.

Tighten
Tighten C-pillar Applique Fasteners to: 4 N·m (35 lb in)

4. Install weatherstrip around rear of roof rail.
5. Install weatherstrip in rear door opening.
6. Close door and verify proper seal and alignment.