For 1990-2009 cars

### Removal Procedure

1. Remove the plastic retainers from the front of the front wheelhouse panel and fascia near the wheelhouse.
2. Remove the lower front plastic retainers.
3. Remove the upper front plastic retainers.
4. Slide the front fascia forward.
5. Remove the front fascia assembly.

### Installation Procedure

1. If installing a new fascia, transfer the following:

• | Upper grille

• | Lower grille

• | Lower deflector

• | Fascia inserts

• | if not equipped with fog lamps, license plate bracket, and support plate.

2. Install the fascia ends over the shoulder bolts extending down from the front fender upper support bracket assembly, and push the fascia back. Holes in the fascia are slotted to allow for installation without removing the bolts. The front fascia lower support plate should be on the lower side of the fascia.
3. Install the plastic retainers from the front of the front wheelhouse panel and fascia near the wheelhouse.
4. Install the upper front plastic retainers.
5. Install the lower front plastic retainers.