For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Slide the front door handle forward and then outward.
3. Twist the door handle to unhook the door handle rod.

### Installation Procedure

1. Twist the door handle to hook the door handle rod into the handle.
2. Install the door handle into the slots and slide rearward.
3. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .