For 1990-2009 cars

### Removal Procedure

1. Insert a small flat-bladed tool between the top corners of the trim panel and the instrument panel (I/P). Pry out the trim panel.
2. Disconnect the electrical connectors.

### Installation Procedure

1. If the center trim plate is being replaced, transfer the electrical switches to the new trim panel.
2. Connect the electrical connectors to the switches.
3. Snap the trim panel into the I/P.