For 1990-2009 cars

The GM of Canada Adhesive Caulking Kit, P/N 10952983, contains the following items:

• | Four different primers

• | A tube of urethane adhesive with a nozzle

• | Four daubers

• | Instructions with warnings

Use the urethane adhesive caulking kit for replacement of any urethane adhesive-installed window using the full cut method.

In the United States or Canada, you may use any of the following equivalent urethane adhesive systems which meet GM Specification GM 3651G:

• | Dow Automotive - Essex 400HV. One part and requires associated primers.

• | Dow Automotive - Essex U216. Two part and requires associated primers.

| Call Dow Automotive at 1-800-453-3779 for more information.

• | 3M™ "Fast Cure" Auto Glass Urethane. One part and requires associated primers.

| Call 3M™ at 1-877-666-2277 for more information.

Use these materials based on specific manufacturer. Do NOT intermix primers or adhesives from one manufacturer to another.

Always follow the system manufacturer's instructions for application, handling, and curing.