For 1990-2009 cars

### Removal Procedure

1. Unsnap the sunshade from the sunshade inner retainer clip.
2. Remove the sunshade fasteners and remove the sunshade.
3. On the illuminated sunshade, disconnect the sunshade wiring connector.

### Installation Procedure

1. On illuminated sunshade, connect the sunshade wiring connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Route the wiring harness into the holes and install the sunshade with fasteners.

Tighten
Tighten the sunshade-to-headliner fasteners to 15 N·m (11 lb ft).

3. Snap the sunshade into the inner retainer clip.