For 1990-2009 cars

### Removal Procedure

1. Remove the cargo shade.
2. Lower the rear seat back assembly.
3. Remove the molding by pulling gently at the attaching clip locations.

### Installation Procedure

1. Position the molding at the attaching clip locations.
2. Secure the molding by pushing gently at the clip locations.
3. Install the cargo shade.
4. Raise the rear seat back assembly.
5. Position the weatherstrip over the cargo shade side cover.