For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Gently remove the hood-to-cowl seal by peeling it up from one end.
3. Use a flat-blade screwdriver to open the filter access door in the cowl leaf screen.
4. Remove any debris in the filter area such as leaves or pine needles.
5. Rotate the locking tabs outward to release the filter assembly.
6. Remove the filter by pulling straight out.

### Installation Procedure

1. Install a new filter noting the air flow direction indicator.
2. Rotate the locking tabs inward to secure the air filter in place.
3. Install the hood-to-cowl seal.
4. Close the cowl leaf screen access door and snap the door closed.