For 1990-2009 cars

### Removal Procedure

1. Move the front seat to the forward most position.
2. Starting at the front of the vehicle, remove the carpet retainer by gently pulling on the retainer at the attaching clip locations.

### Installation Procedure

1. Position the carpet retainer into the vehicle.
2. Starting at the rear of the vehicle, slide the carpet retainer under the rear seat cushion.
3. Position the carpet retainer over the remaining attaching clip locations.
4. Gently push on the attaching clips to install the carpet retainer.
5. Install the weatherstrip over the carpet retainer using a flat-blade tool.