For 1990-2009 cars

### Removal Procedure

1. Pull control assembly boot down to disengage boot from knob.
2. Using a screwdriver, remove control lever knob retainer. Remove control lever knob.
3. Pull up on control boot until indicator bezel disengages from console.
4. Disconnect indicator bezel electrical connector. Remove bezel and boot.
5. Disengage control boot from indicator bezel from underside of bezel. Remove boot.

### Installation Procedure

1. Install control boot into indicator bezel.
2. Install bezel and boot over shift lever and connect indicator bezel electrical connector. Snap bezel into console opening.
3. Install control lever knob and knob retainer.
4. Install control assembly boot onto knob so O-ring in top of boot is seated in groove on bottom of knob.