For 1990-2009 cars

Table 1: | A/C Compressor Clutch -- A/C Compressor
Table 2: | A/C Pressure Sensor -- Engine Compartment - Right
Table 3: | Blower Motor
Table 4: | Blower Motor Resistor Assembly
Table 5: | HVAC Control Module C1
Table 6: | HVAC Control Module C2
Table 7: | Mode Actuator
Table 8: | Recirculation Door Actuator

#### A/C Compressor Clutch -- A/C Compressor

Connector Part Information |

• | 12052644

• | Gray

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | BLK | 150 | Black
B | DK GRN | 59 | A/C Relay

#### A/C Pressure Sensor -- Engine Compartment - Right

Connector Part Information |

• | 12110192

• | Black

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | BLK | 552 | PCM (L81)
BLK | 2759 | LIPFB (L61)
B | GRY | 596 | PCM (L81)
GRY | 2709 | Fuel Tank Pressure Sensor (L61)
C | RED/BLK | 380 | PCM/ECM

#### Blower Motor

Connector Part Information |

• | 7123-6020

• | 2-Way F Yazaki 58M-Type (Natural)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 550 | Ground
B | YEL | 268 | Blower Motor Supply Voltage

#### Blower Motor Resistor Assembly

Connector Part Information |

• | 12129566

• | 4-Way F MP280 SLD (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 65 | Medium 1 Blower Motor Supply Voltage
B | BLU LT | 72 | Medium 2 Blower Motor Supply Voltage
C | YEL | 268 | Blower Motor Supply Voltage
D | PNK | 908 | Low Blower Motor Supply Voltage

#### HVAC Control Module C1

Connector Part Information |

• | 12084945

• | 16-Way F MP100 (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1-A2 | -- | -- | Not Used
A3 | BLK | 550 | Ground
A4 | -- | -- | Not Used
A5 | PPL | 130 | Ignition 3 Voltage
A6 | WHT | 119 | Mode Door Control
A7 | BLK/WHT | 907 | Ground
A8 | -- | -- | Not Used
B1 | GRY | 8 | Instrument Panel Lamp Supply Voltage
B2 | BLU LT | 292 | Rear Defog Switch Signal
B3 | YEL | 60 | Blower Motor Switch Supply Voltage
B4 | ORG | 683 | Rear Defog Indicator Supply Voltage
B5 | GRN LT | 66 | A/C Request Signal
B6 | GRN LT/BLK | 906 | Recirculation Door, Recirculation Feed
B7 | BRN | 641 | Ignition 3 Voltage
B8 | BLU LT/WHT | 905 | Recirculation Door, Fresh Air Feed

#### HVAC Control Module C2

Connector Part Information |

• | 0192F206-00

• | 6-Way F Kantas (White)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YEL | 60 | Blower Motor Switch Supply Voltage
2 | ORG | 52 | High Blower Motor Supply Voltage
3 | BLU LT | 72 | Medium 2 Blower Motor Supply Voltage
4 | PPL | 65 | Medium 1 Blower Motor Supply Voltage
5 | PNK | 908 | Low Blower Motor Supply Voltage
6 | BRN | 341 | Ignition 3 Voltage

#### Mode Actuator

Connector Part Information |

• | 12040953

• | 6-Way F Micro-Pack 100 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
5-6 | -- | -- | Not Used
7 | BLK/WHT | 907 | Ground
8 | WHT | 119 | Mode Door Control
9 | -- | -- | Not Used
10 | PPL | 130 | Ignition 3 Voltage

#### Recirculation Door Actuator

Connector Part Information |

• | 12040953

• | 6-Way F Micro-Pack 100 Series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
5 | BLU LT/WHT | 905 | Recirculation Door, Fresh Air Feed
6 | ORG/BLK | 906 | Recirculation Door, Recirculation Feed
7-10 | -- | -- | Not Used