For 1990-2009 cars

## Dome Lamp Replacement Sedan

### Removal Procedure

1. Insert a flat-bladed tool between the lens and the headliner.
2. Remove the bulbs (1,2,3).
3. Slide the lamp housing to either the left or the right and pull downward.
4. Disconnect the wire connector.

### Installation Procedure

1. Install the wire connector.
2. Install the lamp housing to the headliner.
3. Install the bulbs (1,2,3).
4. Install the lens until the tabs are fully seated.