For 1990-2009 cars

#### Tools Required

J 42067 Rear Main Seal Installer

1. Remove excess sealer from seal recess.
2. Lubricate the outside diameter of the new crankshaft seal with clean engine oil.
3. Using the J 42067 , press the new crankshaft seal into the housing. The J 42067 also establishes the depth of the seal in the crankshaft seal bore.

#### Tools Required

J 42067 Rear Crankshaft Seal Installer

### Installation Procedure

1. Remove the excess sealer from the seal recess.
2. Lubricate the outside diameter of the crankshaft seal with clean engine oil.
3. Press the new crankshaft seal into housing, using the J 42067 . The installer also establishes the depth of the seal in the crankshaft seal bore.