For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor-to-Block Bolt | 25 N·m | 18 lb ft
Air Pipe Bolts | 25 N·m | 18 lb ft
Air Pipe Nut | 16 N·m | 11 lb ft
Balance Shaft Chain Guide (Adjustable) Bolt | 10 N·m | 89 lb in
Balance Shaft Chain Guide (Fixed) Bolts | 10 N·m | 89 lb in
Balance Shaft Chain Guide (Upper) Bolts | 10 N·m | 89 lb in
Balance Shaft Chain Tensioner Bolts | 10 N·m | 89 lb in
Balance Shaft Drive Sprockets | 55 N·m | 41 lb ft
Balance Shaft Retaining Bolts | 10 N·m | 89 lb in
Ball Stud-to-Steering Knuckle Nuts | 100 N·m | 74 lb ft
Battery Terminal Bolts | 17 N·m | 13 lb ft
Cam Cover Bolts-to-Hold J 43649 | 10 N·m | 89 lb in
Camshaft Bearing Cap Bolts | 10 N·m | 89 lb in
Camshaft Cover Bolts | 10 N·m | 89 lb in
Camshaft Cover Ground Strap Fastener | 10 N·m | 89 lb in
Camshaft Sprocket Bolts

- First Pass

85 N·m

63 lb ft

- Final Pass

30 degrees

Connecting Rod Bolts

- First Pass

25 N·m

18 lb ft

- Final Pass

100 degrees

Coolant Jacket Plug | 20 N·m | 15 lb in
Crankshaft Bearing Cap Initial Torque (Lower Crankcase-to-Block Bolts)

- First Pass

20 N·m

15 lb ft

- Final Pass

70 degrees

Crankshaft Damper Pulley Bolt

- First Pass

100 N·m

74 lb ft

- Final Pass

75 degrees

Crankshaft Position Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Pulley Bolt

- First Pass

100 N·m

74 lb ft

- Final Pass

75 degrees

Cylinder Head Air Bleed Tube Fastener | 15 N·m | 11 lb in
Cylinder Head Bolts

- First Pass

30 N·m

22 lb ft

- Final Pass

155 degrees

Cylinder Head Front Bolts | 35 N·m | 26 lb ft
Cylinder Head Front Chaincase Bolts | 20 N·m | 15 lb ft
Cylinder Head Oil Gallery Plug | 35 N·m | 26 lb ft
Degas Hose Bracket Bolt | 10 N·m | 89 lb in
Drive Belt Tensioner Bolt | 45 N·m | 33 lb ft
EGR Cover Bolts | 25 N·m | 18 lb ft
Engine Coolant Temperature Sensor | 20 N·m | 15 lb ft
Engine Harness Bracket Bolts | 10 N·m | 89 lb in
Engine Mount Bracket-to-Engine Bolts | 90 N·m | 66 lb ft
Engine Mount-to-Body Bolts | 55 N·m | 41 lb ft
Engine Mount-to-Engine Mount Bracket Bolts | 55 N·m | 41 lb ft
Exhaust Manifold Heat Shield Bolts | 25 N·m | 18 lb ft
Exhaust Manifold Pipe-to-Exhaust Manifold Nuts | 30 N·m | 22 lb ft
Exhaust Manifold Pipe-to-Resonator Bolts | 20 N·m | 15 lb ft
Exhaust Manifold Studs-to-Cylinder Head | 10 N·m | 89 lb in
Exhaust Manifold-to-Cylinder Head Nuts | 12 N·m | 9 lb ft
Flywheel Bolt

- First Pass

53 N·m

39 lb ft

- Final Pass

25 degrees

Front Cover-to-Block Bolts | 25 N·m | 18 lb ft
Fuel Line Bolt | 10 N·m | 89 lb in
Fuel Rail Bracket Stud | 10 N·m | 89 lb in
Ignition Coil-to-Camshaft Cover Bolts | 8 N·m | 71 lb in
Intake Camshaft Rear Bearing Cap Bolts | 25 N·m | 18 lb ft
Intake Manifold Studs | 6 N·m | 56 lb in
Intake Manifold-to-Cylinder Head Bolts | 10 N·m | 89 lb in
Intake Manifold-to-Cylinder Head Nuts | 10 N·m | 89 lb in
Intake Manifold-to-Cylinder Head Studs | 6 N·m | 60 lb in
Knock Sensor Bolt | 25 N·m | 18 lb in
Knock Sensor-to-Engine Block Bolt | 25 N·m | 18 lb ft
Lower Crankcase-to-Block Peripheral Bolts | 25 N·m | 18 lb ft
Lower Engine-to-Transmission Bell Housing Bolts | 65 N·m | 48 lb ft
Oil Drain Plug | 25 N·m | 18 lb ft
Oil Filter Cap | 25 N·m | 18 lb ft
Oil Gallery Plug | 35 N·m | 26 lb ft
Oil Gallery Plug (Rear) | 60 N·m | 44 lb ft
Oil Level Indicator Tube-to-Intake Manifold Bolt | 10 N·m | 89 lb in
Oil Pan-to-Block Bolts | 25 N·m | 18 lb ft
Oil Pressure Switch | 10 N·m | 89 lb in
Oil pump Gerotor Cover Bolts | 6 N·m | 53 lb in
Oil Pump Pressure Relief Valve Plug | 40 N·m | 3 lb in
Oxygen Sensor Bolts | 30 N·m | 22 lb ft
Power Steering Pump Bolts | 25 N·m | 18 lb ft
Shift Control Rod Pinch Bolt

- First Pass

12 N·m

9 lb ft

- Final Pass

180 degrees

Spark Plugs | 20 N·m | 15 lb ft
Stabilizer Link-to-Strut Assembly | 65 N·m | 50 lb ft
Steering Gear-to-Intermediate Shaft Pinch Bolt | 30 N·m | 22 lb ft
Support Plate-to-Engine Block | 10 N·m | 89 lb in
Suspension Support Bolts

- First Pass

100 N·m

74 lb ft

- Final Pass

45 degrees

Thermostat Housing-to-Block Bolts | 10 N·m | 89 lb in
Throttle Body Bolts | 10 N·m | 89 lb in
Throttle Body Nuts | 10 N·m | 89 lb in
Throttle Body Studs-to-Cylinder Head | 6 N·m | 60 lb in
Tie Rod end Linkage Installer | 45 N·m | 35 lb ft
Tie Rod Nut | 60 N·m | 45 lb ft
Timing Chain Guide (Adjustable) Bolt | 10 N·m | 89 lb in
Timing Chain Guide (Fixed) Bolts | 10 N·m | 89 lb in
Timing Chain Guide (Upper) Bolts | 10 N·m | 89 lb in
Timing Chain Guide Bolt Access Hole Plug | 40 N·m | 30 lb ft
Timing Chain Oil Nozzle Bolt | 10 N·m | 89 lb in
Timing Chain Tensioner Bolts | 75 N·m | 55 lb ft
Torque Converter Bolts | 75 N·m | 55 lb ft
Transmission Nose Bracket Bolts | 35 N·m | 26 lb ft
Upper Bell Housing Bolts | 65 N·m | 48 lb ft
Water Pump Bolts | 25 N·m | 18 lb ft
Wheel Bolts (Final Torque) | 125 N·m | 92 lb ft
Wheel Bolts (Initial Torque) | 63 N·m | 46 lb ft