For 1990-2009 cars

### Removal Procedure

Caution: Always wear heavy gloves and safety glasses when handling glass to minimize the risk of injury.

Notice: Place protective covers on body to prevent paint damage.

1. Remove the center high mount stop lamp cover.
2. Unsnap the center high mount stop lamp from the roof and disconnect the wire connector.
3. Lower the rear half of the headliner. Use lightweight wood or foam blocks to hold the headliner down.
4. Remove the molding around the rear window carefully; try not to excessively stretch it.
5. Remove the electrical connectors from the rear window defogger bus bars. Locate the electrical connectors and mark the location both inside and outside of the window with tape so as not to damage the wiring/connectors when using the power glass removal tool.

Caution: When using power tools that may create smoke when cutting urethane sealant, work should be done in a well ventilated area and/or with a NIOSH/MSHA Approved air supplied respirator to prevent possible harmful exposure.

When the urethane adhesive is heated enough to give off smoke, high levels of methylene diisocyanate (MDI) may be present. Unprotected exposure to methylene diisocyanate (MDI) may result in severe, chronic, debilitating respiratory problems.

Notice: Care must be taken not to damage the roof when using power glass removal tool.

6. With the power glass removal tool, cut the urethane seal along the roof, down the sides, and along the package shelf between the decklid hinges from inside of the vehicle.
7. Use piano wire to cut the urethane at the lower corners. Feed the wire under the glass at the C-pillar through the inside and back out at the package shelf, then around the outside of the bead. Use a sawing motion to cut the urethane.
8. With the aid of a helper, remove the window assembly.

### Installation Procedure

Important: Loose material and/or a rough surface on the remaining urethane may cause sealing problems during installation of the window assembly.

1. Remove the old urethane with a razor knife leaving a thin film, approximately 1-2 mm (0.04-0.08 in) around the perimeter of the window opening and the window assembly, if being reused.
2. Clean the entire window opening and the glass bonding surfaces with a clean, lint-free, alcohol dampened cloth. Allow it to air dry.
3. Install the molding around the perimeter of the glass.

Important: If the applied molding becomes loose from the edge of the glass, clear and black prime the affected area. Allow it to air dry. Apply a thin bead of urethane and install the molding.

4. Replace the molding if damaged or excessively stretched.

Notice: To prevent corrosion, paint damage around the window opening by the power glass removal tool must be covered with pinchweld primer. Do not prime over existing urethane. Follow manufacturers recommendations for drying time.

Important: Shake the glass prep primer, Clear #1, well before using.

5. For a new window assembly only, apply the glass prep primer, Clear #1, around the entire perimeter of the glass using a dauber. Wipe dry with a clean, lint-free cloth

Specifications
The primer area minimum width A is 18 mm (0.71 in).

Important: Shake glass primer, Black #2, well before applying.

6. With a new dauber, apply the glass prep primer, Black #2, around the entire perimeter over Clear #1. Allow the primer to dry 5 minutes before applying the urethane.

Specifications
The primer area minimum width A is 18 mm (0.71 in).

7. Apply a smooth continuous bead of adhesive directly to the old urethane adhesive in the glass opening or to the glass. Apply according to the dimensions shown.

Specifications

• | The bead dimension minimum width B is 10 mm (0.93 in).

• | The bead dimension minimum height C is 14 mm (0.55 in).

8. With the aid of an assistant, lift the glass into the window opening.
9. Align the top edge of the molding with the notches in the roof panel. Make certain the lip of the applied molding laps over the roof feature line.
10. Press the glass firmly to wet-out and set the adhesive. Use care to avoid excessive squeeze out which would cause an appearance problem.
11. Using duct tape, or equivalent, tape the glass up to the roof.
12. Align the glass to the upper reveal molding using the adjusters at the base of the windshield and the center glass side-to-side.

Notice: Until the new urethane has cured, air pressure from a closing door may cause the glass to move. To prevent this, lower the opposite side door window a minimum of 76 mm (3 in) before closing the door.

13. Watertest the vehicle using a soft spray. Use warm or hot water if available. Do not direct a hard stream of water on fresh adhesive material. Water applied on top of the urethane adhesive, either during a watertest or part of a separate operation, will speed up the cure of the urethane.
14. Inspect for leaks from inside of the vehicle. Paddle in extra adhesive at the leak points using a tongue depressor or a similar flat flexible tool.
15. Connect the rear window defogger electrical connectors to the bus bars.
16. Remove the previously installed blocks from underneath the headliner.
17. Install the center high mount stop lamp.

Important: The vehicle must remain at the normal room temperature for 6 hours to complete the proper cure of the adhesive. Refer to the manufacturer's recommendation.

18. Install the center high mount stop lamp cover.