For 1990-2009 cars

### Removal Procedure

1. Remove the fasteners that attach the amplifier to the instrument panel (I/P) beam.
2. Slide the amplifier off of the clutch pedal bracket.
3. Disconnect the electrical connector connectors from the amplifier.
4. Remove the amplifier from the vehicle.

### Installation Procedure

1. Connect the electrical connector connectors to the amplifier.
2. Slide the amplifier onto the clutch pedal bracket.

Notice: Refer to Fastener Notice in the Preface section.

3. Position the amplifier to the I/P beam. Install the fasteners.

Tighten
Tighten the fasteners to 10 N·m (89 lb in).