For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Exhaust Manifold Pipe Heat Shield Bolts (L81) | 8 N·m | 71 lb in
Exhaust Manifold Pipe-to-Exhaust Manifold Nuts | 30 N·m | 22 lb ft
Exhaust Manifold Pipe-to-Exhaust Pipe Bolts | 20 N·m | 15 lb ft
Frame Assembly-to-Body Bolts | 90 N·m + 45-60 degrees | 66 lb ft + 45-60 degrees
Inner Tie Rod-to-Steering Gear | 95 N·m | 70 lb ft
Intermediate Shaft Pinch Bolt | 30 N·m | 22 lb ft
O2 Sensor Clip-to-Underbody Attachment Nut | 4 N·m | 35 lb in
O2 Sensor on Exhaust Manifold Pipe (L81) | 45 N·m | 33 lb ft
Power Steering Fluid Reservoir-to-Radiator Support Attachment Fasteners | 7 N·m | 62 lb in
Power Steering High Pressure Line-to-Pump (L61) | 27 N·m | 20 lb ft
Power Steering High Pressure Line-to-Pump (L81) | 27 N·m | 20 lb ft
Power Steering Lines-to-Steering Gear | 27 N·m | 20 lb ft
Power Steering Pump Pulley-to-Hub Bolt | 20 N·m | 15 lb ft
Power Steering Pump-to-Bracket Bolts (L81) | 20 N·m | 15 lb ft
Power Steering Pump-to-Engine (L61) | 25 N·m | 18 lb ft
Rear Transaxle Mount Through Bolt | 90 N·m | 66 lb ft
Rear Transaxle Mount-to-Frame Bolts | 60 N·m | 44 lb ft
Signal Switch Housing-to-Steering Column Screws | 1.5 N·m | 14 lb in
Stabilizer Bar Link-to-Strut | 65 N·m | 48 lb ft
Steering Column Trim Covers | 4 N·m | 35 lb in
Steering Column-to-Instrument Panel (I/P) Support Beam Fasteners | 30 N·m | 22 lb ft
Steering Gear Adjuster Plug | 12 N·m | 9 lb ft
Steering Gear Heat Shield-to-Frame | 4 N·m | 35 lb in
Steering Gear Pre-Load Adjuster Plug Lock Nut | 70 N·m | 52 lb ft
Steering Gear-to-Frame | 45 N·m + 90-105 degrees | 35 lb ft + 90-105 degrees
Steering Wheel Nut | 40 N·m | 30 lb ft
Suspension Support-to-Body Bolts | 90 N·m + 45-60 degrees | 66 lb ft + 45-60 degrees
Tie Rod End Linkage Installer | 45 N·m | 33 lb ft
Tie Rod End-to-Steering Knuckle Nut | 60 N·m | 44 lb ft
Wheel Bolts

- Initial Torque

63 N·m

46 lb ft

- Final Torque

125 N·m

92 lb ft