For 1990-2009 cars

### Removal Procedure

1. Remove the front door outer belt seal. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .
2. Slide the applique upward to disengage the hooks from the door window frame.
3. Remove the applique from the door window frame by pulling out on the front edge.

### Installation Procedure

1. Position the applique to the slots in the door window frame.

Press the applique to engage the retainers into the door.

2. Slide the applique downward to engage the retainers to the door window frame.
3. Install the front door outer belt seal. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .