For 1990-2009 cars

### Removal Procedure

1. Remove headlamp housing. Refer to "Headlamp Housing" removal procedure in this section.
2. Remove nuts attaching fog lamp bracket to impact bar.
3. Remove fog lamp assembly and bracket down through bottom of front fascia.
4. Remove fog lamp assembly from fog lamp bracket.

### Installation Procedure

1. Install fog lamp assembly to fog lamp bracket.
2. Place fog lamp assembly and bracket into position through bottom of front fascia.
3. Install two nuts attaching fog lamp bracket to impact bar.

Tighten
Tighten Fog Lamp Bracket-to-Impact Bar Fasteners to: 30 N·m (22 lb ft)

4. Install headlamp housing. Refer to "Headlamp Housing" installation procedure in this section.