For 1990-2009 cars

### Removal Procedure

Caution: Ensure that the vehicle is properly supported and squarely positioned. To help avoid personal injury when a vehicle is on a hoist, provide additional support for the vehicle on the opposite end from which the components are being removed.

1. Position the vehicle on a hoist and raise the vehicle.
2. Disconnect the electrical connector.
3. Remove the output speed sensor stud.
4. Remove the output speed sensor from the transaxle case.

Important: Inspect the O-ring for damage and replace if necessary.

5. Remove the O-ring from the output speed sensor.

### Installation Procedure

1. Install the O-ring onto the output speed sensor.
2. Install the output speed sensor into the transaxle case.
3. Install the output speed sensor stud.

Tighten
Tighten the speed sensor stud to 11 N·m (8 lb ft).

4. Connect the electrical connector.
5. Lower the vehicle.