For 1990-2009 cars

### Installation Procedure

1. Install the engine front cover and new gasket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the long water pump bolt.

Tighten
Tighten the water pump bolt to 25 N·m (18 lb ft).

3. Install the engine front cover bolts.

Tighten
Tighten the front cover-to-block bolts to 25 N·m (18 lb ft).

4. Install the accessory drive belt tensioner.

Tighten
Tighten the drive belt tensioner bolt to 45 N·m (33 lb ft).