For 1990-2009 cars

Part Measured | Specification
--- | ---
Metric | English
Bushing, Maximum ID Important: The pump bushing must have a complete burnt-orange color Teflon® coating. If any portion of the Teflon® coating is worn and bronze material is visible, replace the pump. | 58.391 mm | 2.3015 in
Drive Gear, Maximum Side Clearance | 0.066 mm | 0.0026 in
Driven Gear, Between Flats Maximum | 52.165 mm | 2.0537 in
Driven Gear, Minimum OD | 108.987 mm | 4.2908 in
Oil Pump Body Gear Cavity, Maximum ID | 109.216 mm | 4.2988 in
Driven Gear to Oil Pump Body, Maximum Diametrical Clearance | 0.204 mm | 0.0080 in
Driven Gear, Maximum Side Clearance | 0.056 mm | 0.0022 in
Driven Gear/Crescent Tooth, Maximum Clearance | 0.455 mm | 0.0179 in
Oil Pump Body Gear Cavity, Maximum Depth | 24.940 mm | 0.9819 in
Wear Plate, Minimum Thickness | 2.950 mm | 0.1161 in