For 1990-2009 cars

Table 1: | Fuse Block - Underhood Label Usage
Table 2: | Underhood Fuse Block C1
Table 3: | Underhood Fuse Block - C2
Table 4: | Underhood Fuse Block - C3
Table 5: | Underhood Fuse Block - C4 (2.2L)
Table 6: | Underhood Fuse Block - C4 (3.0L)
Table 7: | Underhood Fuse Block C5
Table 8: | Underhood Fuse Block C6
Table 9: | Underhood Fuse Block C7
Table 10: | Fuse Block -I/P- Left - Label Usage
Table 11: | Fuse Block- I/P - Left C1
Table 12: | Fuse Block-- I/P- Left C2
Table 13: | Fuse Block - I/P- Right Label Usage
Table 14: | Fuse Block - Right - I/P C1
Table 15: | Fuse Block - I/P- Right C2

### Fuse Block - Underhood Label

#### Fuse Block - Underhood Label Usage

Fuse | Rating | Description
--- | --- | ---
ABS 2 | 30A | EBTCM
ABS1 | 30A | EBTCM
AC | 10A | AC RELAY
AC RELAY | -- | AC CLUTCH, AC DIODE
A/C DIODE | -- | --
AUX POWER | 20A | AUXILIARY POWER OUTLET
BACKUP/TURN | 10A | HAZARD SW., HDLMP RELAY
BRAKE | 15A | STOP LAMP SW.
BCM/ECM/CRUISE | 10A | CRUISE SW., CRUISE BRAKE SW., CCM, ABS TRACTION CONTROL, ECM(3.0L), BCM, VENT SOLENOID(2.2L)
BCM 2 | 10A | BCM, HVAC CNTRL MODULE
BCM CLUSTER | 15A | BCM, IPC, REAR COMPARTMENT LID RELEASE, DIMMER SW.
COOL FAN 2 | 30A | COOLING FAN CNTRL MODULE
COOL FAN 1 | 30A | COOLING FAN CNTRL MODULE
CONTROLS IGN 1 | 10A | PCM(2.2L), AUTO TRANS(2.2L), COOLING FAN CNTRL MODULE(3.0L)
CONTROLS B+ | 10A | PCM(2.2L), ECM(3.0L), TCM(3.0L)
CRUISE SW | 2A | INFLATABLE RESTRAINT STEERING WHEEL MODULE COIL
CD/DLC | 15A | RADIO, DLC
DRL RELAY | -- | MARKER/HDLMP
ENGINE CNTL 1 (V6) | 10A | AC RELAY, (HO2S)2, (HO2S)1, MAFS, (EVAP) CANISTER PURGE SOLENOID, (EGR)VALVE
ENGINE CNTL 2 (V6) | 10A | MANIFOLD INLINE, VARIABLE INTAKE MANIFOLD FLOP, FUEL INJECTORS
ENGINE CNTL 3 (V6) | 10A | ECM(3.0), (HO2S)1, (HO2S)2, (EVAP) CANISTER VENT SOLENOID,FUEL PUMP RELAY
EIS (L4) | 10A | (HO2S)2, (HO2S)1, ICM, AIR PUMP RELAY
FUSE PULLER | -- | --
FUEL PUMP | 15A | FUEL PUMP RELAY
FUEL PUMP RELAY | -- | FUEL PUMP RELAY
HVAC BLOWER | 40A | IGN3 RELAY
HORN | 10A | HORN RELAY
HORN RELAY | -- | HORN
HAZARD | 15A | HAZARD SW.
IGN 0/3/CR (L4) | 30A | IGN SW.
IGN 0/3/CR (V6) | 30A | IGN SW.
IGN 1/2 | 30A | IGN SW.
INJECTOR (L4) | 10A | (EVAP) CANISTER PURGE SOLENOID, FUEL INJECTORS
IGN (V6) | 15A | IGN COIL(1, 3, 5), IGN COIL(2, 4, 6)
IGN 0 | 10A | PCM(2.2L), IF BOX, ELECTRONIC(PRNDL), PARK LOCK SOLENOID
IGN 1 | 10A | IPC, HVAC LOW COOLANT SW., SDM
IP BATT RT | 30A | PREM AMP, DOORLOCKS, BODY, FOGLAMP, PWR SEAT
LT HEADLAMP | 10A | DRL RELAY, HDLMP
LIGHTER | 20A | AUXILIARY POWER OUTLET
MAIN RELAY (V6) | -- | ENG CNTRL1, ENG CNTRL2, ENG CNTRL3
PARK LAMP | 10A | PARK LAMP RELAY
RT HEADLAMP | 10A | HDLMP
REAR WIPER RELAY | -- | WIPER MOTOR-RR
RADIO | 10A | RADIO
REAR DEFOG | 25A | REAR DEFOG RELAY
WDO/SUNRF (V6) | 30A | WINDOW RELAY, SUNROOF MODULE
WDO/SUNRF (L4) | 30A | AIR PUMP RELAY, WINDOW RELAY, SUNROOF ASSEMBLY
WIPER RELAY | -- | WINSHIELD WIPER/WASHER SW.

### Fuse Block - Underhood Top View (3.0L)

### Fuse Block - Underhood Top View (2.2L)

### Fuse Block - Underhood Bottom View

#### Underhood Fuse Block C1

Connector Part Information |

• | 15319797

• | 2-Way F (L-GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | RD | 202 | Battery Positive Voltage
B | RD | 1202 | Battery Positive Voltage

#### Underhood Fuse Block - C2

Connector Part Information |

• | 15328719

• | 68-Way F (BN)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1-A2 | -- | -- | Not Used
A3 | D-BU | 1201 | Headlamp Low Beam Ground (3.0L)
A4 | -- | -- | Not Used
A5 | D-BU | 473 | High Speed Cooling Fan Relay Control
A6-A7 | -- | -- | Not Used
A8 | PK | 839 | Ignition 1 Voltage (3.0L)
A9-A10 | -- | -- | Not Used
A11 | BK | 150 | Ground
A12 | D-GN | 335 | Cooling Fan Relay Control
B1-B8 | -- | -- | Not Used
B9 | BN | 9 | Park Lamp Supply Voltage
B10-C2 | -- | -- | Not Used
C3 | D-BU | 1201 | Headlamp Low Beam Ground (3.0L)
C4-C8 | -- | -- | Not Used
C9 | BN | 9 | Park Lamp Supply Voltage
C10-C12 | -- | -- | Not Used
D1 | OG | 40 | Battery Positive Voltage
D2 | D-BU | 545 | DRL Supply Voltage
D3 | -- | -- | Not Used
D4 | D-GN | 29 | Horn Control
D5-D12 | -- | -- | Not Used
D5 | -- | -- | Not Used
D9 | BN | 9 | Park Lamp Supply Voltage
E1 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage (3.0L)
BK/WH | 99 | Windshield Washer Fluid Level Signal (2.2L)
E2 | -- | -- | Not Used
E3 | D-BU | 1201 | Headlamp Low Beam Ground (2.2L)
PK | 1200 | Headlamp High Beam Ground (3.0L)
E4 | -- | -- | Not Used
E5 | PU | 34 | Fog Lamp Supply Voltage (T96)
E6 | D-GN | 392 | Rear Window Washer Switch Signal (3.0L)
PK | 1200 | Headlamp High Beam Signal
E7-E12 | -- | -- | Not Used
F1 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
F2 | -- | -- | Not Used
F3 | D-BU | 1201 | Headlamp Low Beam Ground (2.2L)
PK | 1200 | Headlamp High Beam Signal (3.0L)
F4 | -- | -- | Not Used
F5 | PU | 34 | Fog Lamp Supply Voltage (T96)
F6 | BK/WH | 99 | Windshield Washer Fluid Level Signal (2.2L)
PK | 1200 | Headlamp High Beam Ground (3.0L)
F7 | RD | 228 | Front Window Washer Switch Signal (2.2L)
F8 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage (2.2L)
RD | 228 | Front Window Washer Switch Signal (3.0L)
F9 | D-GN | 392 | Rear Window Washer Switch Signal (2.2L)
F10 | OG | 140 | Battery Positive Voltage
F11-F12 | -- | -- | Not Used

#### Underhood Fuse Block - C3

Connector Part Information |

• | 15303512

• | Gray

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
A2 | OG | 300 | Ignition 3 Voltage (2.2L)
D-BU | 1201 | Headlamp Low Beam Ground (3.0L)
A3 | WH | 393 | Rear Window Wiper Motor Control
A4 | -- | -- | Not Used
A5 | PU | 34 | Fog Lamp Supply Voltage
A6 | PU | 1500 | Ignition 0 Voltage
PU | 1500 | Ignition 0 Voltage (w/ A/T)
A7 | RD | 402 | Battery Positive Voltage (2.2L)
RD | 302 | Battery Positive Voltage (3.0L)
A8 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage (2.2L)
RD | 228 | Windshield Washer Pump Signal (3.0L)
RD | 228 | Windshield Washer Pump Signal (3.0L)
A9 | BN | 741 | Ignition 3 Voltage
A10 | OG | 540 | Battery Positive Voltage
A11 | L-BU | 97 | Windshield Wiper Switch Mist/Off/Low Signal
A12 | -- | -- | Not Used
B1 | BK/WH | 99 | Windshield Washer Fluid Level Signal (2.2L)
B2 | BK/WH | 1579 | Oil Life Reset Switch Signal (2.2L)
L-BU | 14 | Left Turn Signal Lamps Supply Voltage (3.0L)
B3 | OG/BK | 1445 | BCM Program Enable Signal
B4 | YE | 143 | Accessory Voltage
B5 | L-BU | 20 | Stop Lamp Supply Voltage
B6 | D-GN | 500 | Ignition 0 Voltage
B7 | RD | 228 | Windshield Washer Pump Signal (2.2L)
RD | 228 | Windshield Washer Pump Signal (2.2L)
D-GN | 392 | Rear Window Washer Switch Signal (3.0L)
D-GN | 392 | Rear Window Washer Switch Signal (3.0L)
B8 | BN | 9 | Park Lamp Supply Voltage (2.2L)
B9 | PK | 339 | Ignition 1 Voltage
B10 | -- | -- | Not Used
B11 | OG/BK | 1445 | BCM Program Enable Signal
B12 | YE | 343 | Accessory Voltage
C1 | L-BU | 832 | Traction Control Active Signal (2.2L w/ABS)
C2 | OG | 1640 | Battery Positive Voltage
OG | 1640 | Battery Positive Voltage (C68)
C3 | D-BU/WH | 1201 | Headlamp Low Beam Ground (2.2L)
D-BU/WH | 1201 | Headlamp Low Beam Ground (2.2L)
WH | 1579 | OIl Life Reset Switch Signal (3.0L)
C4 | -- | -- | Not Used
C5 | PK | 1200 | Headlamp High Beam Ground (2.2L)
C8 | D-GN | 392 | Washer Pump Supply Voltage (2.2L)
BN | 9 | Park Lamp Supply Voltage (3.0L)
C9 | PK | 339 | Ignition 1 Voltage (2.2L)
C10 | -- | -- | Not Used
C11 | OG | 440 | Battery Positive Voltage
C12 | GY | 120 | Fuel Pump Supply Voltage (2.2L)
D1 | L-GN/BK | 592 | DRL Relay Control
D2 | -- | -- | Not Used
D3 | BN | 1341 | Ignition 3 Voltage (M/T)
BK | 28 | Horn Relay Control (3.0L)
BK | 28 | Horn Relay Control (3.0L)
D4 | OG | 1440 | Battery Positive Voltage
D5 | PK | 1200 | Headlamp High Beam Ground (2.2L)
PK | 1200 | Headlamp High Beam Ground (2.2L)
BK/WH | 771 | Transmission Range Switch Signal A (3.0L)
D8 | PK | 239 | Ignition 1 Voltage (3.0L)
PK | 239 | Ignition 1 Voltage (3.0L)
D9 | -- | -- | Not Used
D10 | PK | 1139 | Ignition 1 Voltage
D11 | -- | -- | Not Used
D12 | L-GN | 120 | Fuel Pump Supply Voltage (3.0L)
E1 | OG | 2240 | Battery Positive Voltage
E2 | -- | -- | Not Used
E3 | BK | 28 | Horn Relay Control (2.2L)
BK | 28 | Horn Relay Control (2.2L)
PK | 1200 | Headlamp High Beam Ground (3.0L)
E4 | OG | 1740 | Battery Positive Voltage
E5 | -- | -- | Not Used
E6 | PK | 2192 | Traction Ready Indicator Control (2.2L w/ ABS)
E7 | OG | 1240 | Battery Positive Voltage
E8 | PK | 239 | Instrument Panel Lamp Control (2.2L)
PK | 239 | Instrument Panel Lamp Control (2.2L)
GY | 773 | Transmission Range Switch Signal C (3.0L)
E9 | PK | 3 | Ignition 1 Voltage
E10 | OG | 1040 | Battery Positive Voltage
E11 | OG | 2540 | Battery Positive Voltage
E12 | GY | 773 | Transmission Range Switch Signal C (2.2L w/ A/T)
L-GN | 24 | Backup Lamp Supply Voltage (3.0L)
F1 | -- | -- | Not Used
F2 | OG | 240 | Battery Positive Voltage
F3 | PK | 39 | Ignition 1 Voltage (2.2L)
PK | 39 | Ignition 1 Voltage (2.2L)
PK | 1200 | Headlamp High Beam Ground (3.0L)
PK | 1200 | Headlamp High Beam Ground (3.0L)
F4 | -- | -- | Not Used
F5 | OG | 2140 | Battery Positive Voltage
OG | 2140 | Battery Positive Voltage
F6 | L-GN | 24 | Backup Lamp Supply Voltage (2.2L)
BK/WH | 99 | Windshield Washer Fluid Level Signal (3.0L)
F7 | -- | -- | Not Used
F8 | BK/WH | 867 | ABS Indicator Failure Control (2.2L w/ABS)
PK | 39 | Ignition 1 Voltage (3.0L)
PK | 39 | Ignition 1 Voltage (3.0L)
F9 | BK/WH | 771 | Transmission Range Switch Signal A (2.2L w/ A/T)
OG | 2740 | Battery Positive Voltage (3.0L)
F10-F11 | -- | -- | Not Used
F12 | OG | 2540 | Battery Positive Voltage
OG | 2540 | Battery Positive Voltage

#### Underhood Fuse Block - C4 (2.2L)

Connector Part Information |

• | 15303513

• | Black

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1-A2 | -- | -- | Not Used
A3 | YE | 772 | Transmission Range Switch Signal B (A/T)
A4 | L-BU | 20 | Stop Lamp Supply Voltage (A/T)
A5 | -- | -- | Not Used
A6 | PU | 415 | AIR Solenoid Supply Voltage
A7 | BK | 150 | Ground (NC1)
A8 | BK | 150 | Ground
A9 | PK | 839 | Ignition 1 Voltage
A10 | -- | -- | Not Used
A11 | L-GN | 867 | ABS Indicator Failure Control (w/ ABS)
A12 | WH | 776 | Transmission Range Switch Signal P (A/T)
WH | 776 | Transmission Range Switch Signal P (A/T)
B1-B2 | -- | -- | Not Used
B3 | YE | 772 | Transmission Range Switch Signal B (A/T)
B4 | L-BU | 20 | Stop Lamp Supply Voltage (w/ ABS)
B5-B9 | -- | -- | Not Used
B10 | PK | 139 | Ignition 1 Voltage
B11 | -- | -- | Not Used
B12 | WH | 776 | Transmission Range Switch Signal P (A/T)
C1-C3 | -- | -- | Not Used
C4 | GN/WH | 459 | A/C Compressor Clutch Relay Control
C5 | -- | -- | Not Used
C6-C7 | -- | -- | Not Used
C8 | BK | 150 | Ground (w/ ABS)
C9 | PK | 839 | Driver Mirror Motor Right Control (A/T)
C10 | PK | 139 | Ignition 1 Voltage
C11 | PU | 1500 | Ignition 0 Voltage
C12 | BK/WH | 771 | Transmission Range Switch Signal A (A/T)
D1-D5 | -- | -- | Not Used
D8 | BK | 150 | Ground
D9-D10 | -- | -- | Not Used
D11 | GY | 773 | Transmission Range Switch Signal C (A/T)
D12 | BK/WH | 771 | Transmission Range Switch Signal A (A/T)
E1 | L-BU | 832 | Traction Control Active Signal (w/ ABS)
E2 | -- | 2192 | Traction Ready Indicator Control (w/ ABS)
E3 | -- | -- | Not Used
E4 | D-GN | 59 | A/C Compressor Clutch Supply Voltage
E5 | PK | 1639 | Ignition 1 Voltage
E6 | BK | 150 | Ground
E7 | -- | -- | Not Used
E8 | BK | 150 | Ground (w/ ABS)
E9 | PK | 239 | Ignition 1 Voltage (A/T)
E10 | PK | 339 | Ignition 1 Voltage (w/ ABS)
E11 | GY | 773 | Transmission Range Switch Signal C (A/T)
E12 | BK | 196 | Windshield Wiper Motor Park Switch Signal
F1-F2 | -- | -- | Not Used
F3 | L-GN | 24 | Backup Lamp Supply Voltage
F4 | OG | 480 | Battery Positive Voltage
F5 | D-BU | 473 | Cooling Fan 2 Relay Control
F6 | BK/WH | 78 | AIR Pump Supply Voltage (M/T)
F7 | -- | 436 | AIR Pump Relay Control (M/T)
F8 | BK | 150 | Ground (M/T)
F9 | PK | 239 | Ignition 1 Voltage (M/T)
F10 | PK | 1639 | Ignition 1 Voltage
PK | 1639 | Ignition 1 Voltage
F11 | BK | 465 | Fuel Pump Relay Control
F12 | D-GN | 335 | Cooling Fan 1 Relay Control

#### Underhood Fuse Block - C4 (3.0L)

Connector Part Information |

• | 15303513

• | Black

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1-A2 | -- | -- | Not Used
A3 | YE | 772 | Transmission Range Switch Signal B
A4 | OG | 2640 | Battery Positive Voltage
A5 | -- | -- | Not Used
A6 | PK | 339 | Ignition 1 Voltage (w/ ABS)
A7 | BN | 582 | TAC Motor Control - 2
BN | 582 | TAC Motor Control - 2
A8 | BK | 150 | Ground
A9 | L-BU | 20 | Stop Lamp Supply Voltage
A10 | L-BU | 20 | Stop Lamp Supply Voltage (w/ ABS)
A11 | BK | 196 | Windshield Wiper Motor Park Switch Signal
A12 | WH | 776 | Transmission Range Switch Signal P
WH | 776 | Transmission Range Switch Signal P
B1 | -- | -- | Not Used
B2 | OG | 2440 | Battery Positive Voltage
B3 | YE | 772 | Transmission Range Switch Signal B
B4 | BK/WH | 771 | Transmission Range Switch Signal A
B5 | -- | -- | Not Used
B6 | PK | 339 | Ignition 1 Voltage
B7 | BN | 582 | TAC Motor Control - 2
B8 | BK | 150 | Ground (w/ ABS)
B9 | -- | -- | Not Used
B10 | L-BU | 20 | Stop Lamp Supply Voltage
B11 | BK/WH | 251 | EGR Solenoid Control
B12 | WH | 776 | Transmission Range Switch Signal P
C1-C3 | -- | -- | Not Used
C4 | GN/WH | 459 | A/C Compressor Clutch Relay Control
C5 | OG | 2740 | Battery Positive Voltage
C6-C7 | -- | -- | Not Used
C8 | BK | 150 | Ground
C9 | PK | 839 | Driver Mirror Motor Right Control
C10 | L-GN | 497 | Fuel Pump Relay Control
C11 | BK/WH | 251 | Ground
C12 | L-GN | 24 | Backup Lamp Supply Voltage
D1 | OG | 480 | Battery Positive Voltage
D2-D5 | -- | -- | Not Used
D8 | BK | 150 | Ground
D9-D10 | -- | -- | Not Used
D11 | BK/WH | 251 | Ground
D12 | YE | 581 | TAC Motor Control - 1
E1 | GY | 2561 | PTO Supply Voltage
E2 | -- | -- | Not Used
E3 | OG | 2440 | Battery Positive Voltage
OG | 2440 | Battery Positive Voltage
E4 | D-GN | 59 | A/C Compressor Clutch Supply Voltage
E5 | OG | 2740 | Battery Positive Voltage
E6 | OG | 2740 | Battery Positive Voltage
E7 | OG | 2740 | Battery Positive Voltage
E8 | BK | 150 | Ground (w/ABS)
E9 | PK | 239 | Ignition 1 Voltage
E10 | PK | 1539 | Ignition 1 Voltage
E11 | GY | 773 | Transmission Range Switch Signal C
E12 | YE | 581 | TAC Motor Control - 1
YE | 581 | TAC Motor Control - 1
F2 | OG | 2440 | Battery Positive Voltage
OG | 2440 | Battery Positive Voltage
F3 | OG | 2640 | Battery Positive Voltage
F4 | BK/WH | 771 | Transmission Range Switch Signal A
F5 | D-BU | 473 | Cooling Fan 2 Relay Control
F6 | -- | -- | Not Used
F7 | OG | 2740 | Battery Positive Voltage
F8 | BK | 150 | Ground
F9 | PU | 1500 | Ignition 0 Voltage
PU | 1500 | Ignition 0 Voltage (w/o ABS)
F10 | PK | 1539 | Ignition 1 Voltage
F11 | GY | 773 | Transmission Range Switch Signal C
F12 | D-GN | 335 | Cooling Fan 1 Relay Control

#### Underhood Fuse Block C5

Connector Part Information |

• | 15319799

• | 2-Way F (GN)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | RD | 702 | Battery Positive Voltage
B | RD | 1002 | Battery Positive Voltage

#### Underhood Fuse Block C6

Connector Part Information |

• | 15319798

• | 2-Way F (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | RD | 102 | Battery Positive Voltage
B | RD | 502 | Battery Positive Voltage

#### Underhood Fuse Block C7

Connector Part Information |

• | 15319800

• | 2-Way F (BN)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | RD | 302 | Battery Positive Voltage (2.2L)
RD | 402 | Battery Positive Voltage (3.0L)

### Fuse Block -I/P- Left - Label

#### Fuse Block -I/P- Left - Label Usage

Fuse | Rating | Description
--- | --- | ---
BTSI/BCM MIRROR | 10A | MIRROR SW., BCM, PARKLOCK SW./BTSI SOLENOID
DIMMER | 10A | IPC, RADIO, TC SW., HTD SEAT SW., REAR COMPARTMENT LID RELEASE AND I/P LAMP DIMMER, HAZARD SW., ELECTRONIC(PRNDL), HVAC CNTRL MODULE,
DEFOG LED | 10A | MIRROR RELAY, HVAC CNTRL MODULE
FUSE PULLER | -- | --
IGN 3 RELAY | -- | IGN3, HVAC CNTRL MODULE
IGN 3 | 10A | HVAC CNTRL MODULE, TC SW., HTD SEAT SW.
REAR DEFOG RELAY | -- | HVAC CNTRL MODULE, TC SW., HTD SEAT SW.
RR COMP | DIODE | --
RADIO | 10A | RADIO
WIPER | 25A | WINSHIELD WIPER MOTOR, WINSHIELD WIPER/WASHER SW., FRONT WIPER RELAY

### Fuse Block -I/P-Left -- Top View

#### Fuse Block- I/P - Left C1

Connector Part Information |

• | 15303512

• | 68-Way F Metri-Pack 280 (L-GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1 | BK | 550 | Ground
BK | 550 | Ground
A2 | -- | -- | Not Used
A3 | BK/WH | 56 | Rear Compartment Lid Release Switch Signal
BK/WH | 1576 | Trunk Release Switch Signal
A4 | OG | 1732 | Courtesy Lamps Supply Voltage
OG | 1732 | Courtesy Lamps Supply Voltage
A5 | GY | 8 | Instrument Panel Lamp Supply Voltage
GY | 8 | Instrument Panel Lamp Supply Voltage
A6 | GY | 8 | Instrument Panel Lamp Supply Voltage
GY | 8 | Instrument Panel Lamp Supply Voltage
A7 | PU | 1319 | Engine/Radio Serial Data K-Line (3.0L)
PU | 1319 | Engine/Radio Serial Data K-Line (3.0L)
A8 | GY | 8 | Instrument Panel Lamp Supply Voltage
A9 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
L-BU | 14 | Left Turn Signal Lamps Supply Voltage
A10 | BK | 2759 | Low Reference
A11 | RD | 502 | Battery Positive Voltage
A12 | OG | 300 | Ignition 3 Voltage
B1 | BK | 550 | Ground
BK | 550 | Ground
B2 | -- | -- | Not Used
B3 | YE | 343 | Accessory Voltage
B4 | OG | 240 | Battery Positive Voltage
B5 | -- | -- | Not Used
B6 | GY | 8 | Instrument Panel Lamp Supply Voltage
GY | 8 | Instrument Panel Lamp Supply Voltage
B7 | PU | 1319 | (3.0L)
B8 | GY | 8 | Instrument Panel Lamp Supply Voltage
GY | 8 | Instrument Panel Lamp Supply Voltage
B9 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
L-BU | 14 | Left Turn Signal Lamps Supply Voltage
B10 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
D-BU | 15 | Right Turn Signal Lamps Supply Voltage
B11 | BK | 550 | Ground
B12 | OG | 300 | (2.2L)
C1-C2 | -- | -- | Not Used
C3 | YE | 343 | Accessory Voltage
C4 | OG | 1732 | Courtesy Lamps Supply Voltage
C5 | OG | 9 | Park Lamp Supply Voltage
OG | 9 | Park Lamp Supply Voltage (A/T)
C8 | GY | 691 | Headlamp Low Beam Relay Control
C9 | PK | 239 | Ignition 1 Voltage
C10 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
D-BU | 15 | Right Turn Signal Lamps Supply Voltage
C11 | BK | 550 | Ground
BK | 550 | Ground
C12 | YE | 268 | Blower Motor High Speed Supply Voltage
D1 | BK | 550 | Ground
D2 | PK | 339 | Ignition 1 Voltage (2.2L)
OG | 2740 | Battery Positive Voltage (3.0L)
D3 | YE | 343 | Accessory Voltage
D4 | WH | 1080 | Park Lamp Relay Control
D5 | BN | 9 | Park Lamp Supply Voltage
BN | 9 | Park Lamp Supply Voltage
D8 | GY | 120 | Fuel Pump Supply Voltage
D9 | -- | -- | Not Used
D10 | BK | 2759 | Low Reference (3.0L)
BK | 2759 | Low Reference (3.0L)
D11 | BK | 550 | Ground
BK | 550 | Ground
D12 | WH | 393 | Rear Window Wiper Motor Control
E1 | BK | 550 | Ground
BK | 550 | Ground
E2 | BN | 9 | Park Lamp Supply Voltage
E3 | BN | 4 | Accessory Voltage
E4 | GY/BK | 745 | Left Front Door Ajar Switch Signal
E5 | L-GN | 24 | Backup Lamp Supply Voltage
E6 | -- | -- | Not Used
E7 | WH | 1310 | EVAP Canister Vent Solenoid Control
E8 | WH | 352 | Fog Lamp Relay Control Circuit
E9 | -- | -- | Not Used
E10 | L-BU | 20 | (2.2L)
E11 | WH | 193 | ear Defog Relay Control
E12 | BN | 641 | Ignition 3 Voltage
F1 | BK | 550 | Ground
F2 | YE | 43 | Accessory Voltage
F3 | BN | 4 | Accessory Voltage
F4 | YE | 743 | Accessory Voltage
YE | 743 | Accessory Voltage
F5 | TN | 683 | Rear Defog Indicator Supply Voltage
F6 | -- | -- | Not Used
F7 | BN | 641 | Ignition 3 Voltage
F8 | PU | 30 | Fuel Level Sensor Signal
F9 | GY | 8 | Instrument Panel Lamp Supply Voltage
F10 | L-BU | 20 | Stop Lamp Supply Voltage
L-BU | 20 | Stop Lamp Supply Voltage
F11 | OG | 1240 | Battery Positive Voltage
F12 | BN | 641 | Ignition 3 Voltage

#### Fuse Block-- I/P- Left C2

Connector Part Information |

• | 15326717

• | Gray

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1 | BK | 550 | Ground
A2 | BN | 9 | Park Lamp Supply Voltage
BN | 9 | Park Lamp Supply Voltage
A3 | BK | 305 | Trunk / Liftgate Key Switch Signal (Wagon)
A4 | YE | 743 | Accessory Voltage
A8 | PU | 30 | Fuel Level Sensor Signal
A9 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
A10 | L-BU | 20 | Stop Lamp Supply Voltage
L-BU | 20 | Stop Lamp Supply Voltage
A12 | PU | 293 | Rear Defog Element Supply Voltage
B1 | BK | 550 | Ground
BK | 550 | Ground
B2 | BN | 9 | Park Lamp Supply Voltage
BN | 9 | Park Lamp Supply Voltage (Wagon)
B3 | -- | -- | Not Used
B4 | L-GN | 24 | Backup Lamp Supply Voltage
L-GN | 24 | Backup Lamp Supply Voltage
B5 | OG | 1732 | Courtesy Lamps Supply Voltage
B8 | WH | 1310 | EVAP Canister Vent Solenoid Control
B9 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
B10 | L-BU | 20 | Stop Lamp Supply Voltage
B11 | OG | 393 | Rear Window Wiper Motor Control (Wagon)
B12 | L-BU | 82 | Mirror Motor Left/Down Control
L-BU | 82 | Mirror Motor Left/Down Control
C1 | OG | 2740 | Battery Positive Voltage
C2 | GY/BK | 745 | Left Front Door Ajar Switch Signal
C3 | -- | -- | Not Used
C4 | TN | 683 | Mirror Relay Coil Supply Voltage
C5-C8 | -- | -- |
C9 | GY | 120 | Fuel Pump Supply Voltage
C10 | -- | -- | Not Used
C11 | BK | 2759 | Low Reference
BK | 2759 | Low Reference
C12 | L-BU | 82 | Mirror Motor Left/Down Control

### Fuse Block - I/P- Right Label

#### Fuse Block - I/P- Right Label Usage

Fuse | Rating | Description
--- | --- | ---
BODY | 10A | MIRROR RELAY, DOOR LOCK SW., TAIL GATE LATCH(WAG)
DR UNLOCK RELAY | -- | --
FOG LAMP | 10A | FOG LAMP RELAY
FOG LAMP RELAY | -- | FOG LAMP
FUSE PULLER | -- | --
HTD SEAT | 20A | HEATED SEAT
LOCKS | 15A | DOOR UNLOCK RELAY, DOOR LOCK RELAY
LOCK RELAY | -- | DOOR LOCK ACTUATOR
MIRROR RELAY | -- | OUT SIDE REARVIEW MIRROR(OSRVM)
PREM AMP | 15A | PREMIUM AMPLIFIER, VCIM
POWER SEAT | 20A | HEATED SEAT SW.
RR WIPER/SUNROOF | 20A | SUNROOF ASS., WIPER MOTOR-RR, REAR WIPER RELAY
UNLOCK RELAY | -- | DOOR LOCK ACTUATOR
WINDOW RELAY | -- | WINDOW SW.

### Fuse Block - I/P- Right Top View

#### Fuse Block - Right - I/P C1

Connector Part Information |

• | 15303512

• | 68-Way F Metri-Pack 280 (L-GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1-B8 | -- | -- | Not Used
B9 | BN | 9 | Park Lamp Supply Voltage
B10-C1 | -- | -- | Not Used
C2 | WH | 194 | Door Unlock Relay Coil Supply Voltage
C3-C4 | -- | -- | Not Used
C5 | OG | 1340 | Battery Positive Voltage (UE1)
C8 | PU | 34 | Fog Lamp Supply Voltage
C9 | BN | 9 | Park Lamp Supply Voltage
C10-D5 | -- | -- | Not Used
D8 | RD | 402 | Battery Positive Voltage
D9 | OG/BK | 781 | Driver Door Lock Switch Unlock Signal
D10 | -- | -- | Not Used
D11 | BN | 4 | Accessory Voltage
D12-E3 | -- | -- | Not Used
E4 | RD/BK | 780 | Driver Door Lock Switch Lock Signal
E5 | OG | 300 | Ignition 3 Voltage
E6-E7 | -- | -- | Not Used
E8 | YE | 317 | Fog Lamp Relay Control Circuit
E9 | -- | -- | Not Used
E10 | PK/BK | 1503 | Passenger Heated Seat High/Low Signal
E11 | YE | 143 | Accessory Voltage
E12-F1 | -- | -- | Not Used
F2 | L-GN | 1391 | Driver Door Unlock Relay Control
F3 | -- | -- | Not Used
F4 | L-BU | 195 | Door Lock Control
F5 | OG | 300 | Ignition 3 Voltage
F6 | -- | -- | Not Used
F7 | OG | 1440 | Battery Positive Voltage
F8-F9 | -- | -- | Not Used
F10 | L-GN | 559 | Passenger Heated Seat On Signal
F11-F12 | -- | -- | Not Used

#### Fuse Block - I/P- Right C2

Connector Part Information |

• | 15326717

• | 30-Way F Metri-Pack 280 (GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1 | BK | 450 | Ground
BK | 450 | Ground
A2 | TN | 694 | Driver Door Lock Actuator Unlock Control
A3 | -- | -- | Not Used
A4 | GY | 295 | Door Lock Actuator Lock Control
A5 | BN | 141 | Ignition 3 Voltage
BN | 141 | Ignition 3 Voltage
A8 | OG | 1340 | Battery Positive Voltage (U67)
A9 | -- | -- | Not Used
A10 | L-GN | 559 | Passenger Heated Seat On Signal
A11 | -- | -- | Not Used
A12 | OG | 267 | Heated Mirror Element Supply Voltage
OG | 267 | Heated Mirror Element Supply Voltage
B1 | -- | -- | Not Used
B2 | TN | 294 | Door Lock Actuator Unlock Control
TN | 294 | Door Lock Actuator Unlock Control
B3 | -- | -- | Not Used
B4 | GY | 295 | Door Lock Actuator Lock Control
GY | 295 | Door Lock Actuator Lock Control
B5 | OG | 640 | Battery Positive Voltage
B8 | -- | -- | Not Used
B9 | OG | 340 | Battery Positive Voltage
OG | 340 | Battery Positive Voltage
B10 | YE | 243 | Accessory Voltage
B11 | -- | -- | Not Used
B12 | YE | 143 | Accessory Voltage
C1 | TN | 683 | Rear Defog Indicator Supply Voltage
C2 | TN | 294 | Door Lock Actuator Unlock Control
C3 | -- | -- | Not Used
C4 | GY | 295 | Door Lock Actuator Lock Control
C5 | OG/BK | 780 | Driver Door Lock Switch Lock Signal
OG/BK | 780 | Driver Door Lock Switch Lock Signal
C8 | BK | 402 | Battery Positive Voltage (Sedan)
C9 | RD/BK | 781 | Driver Door Lock Switch Unlock Signal
RD/BK | 781 | Driver Door Lock Switch Unlock Signal
C10 | YE | 243 | Accessory Voltage
C11 | PK/BK | 1503 | Passenger Heated Seat High/Low Signal
C12 | OG | 340 | Battery Positive Voltage (Wagon)