For 1990-2009 cars

### Removal Procedure

1. Lower the screen from the console.
2. Remove the dome light lens cover.
3. Remove the bulbs from the dome light.
4. Remove the screws from behind the screen.
5. Remove the screws from the dome light.
6. Disconnect the electrical connectors from the overhead console.
7. Remove the overhead console from the headliner.

### Installation Procedure

1. Connect the electrical connectors to the console.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screws to the dome light.

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the screws to the rear of the DVD screen.

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. Install the bulbs in the dome light.
5. Install the dome light lens cover.
6. Raise the screen and lock the screen into place.