For 1990-2009 cars

### Removal Procedure

1. Remove the pull handle plugs to expose the pull handle fasteners.
2. Remove the fasteners and remove the pull handle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Position the pull handle and install the pull handle fasteners.

Tighten
Tighten the fasteners to 5 N·m (44 lb in).

2. Install the pull handle plugs.