For 1990-2009 cars

### Removal Procedure

1. Remove the bolts from the wheelhouse liner.
2. Remove the inner push-in retainers from the wheelhouse liner.
3. Remove the wheelhouse liner from the front fender.

### Installation Procedure

1. Position the wheelhouse liner to the front fender.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts to the wheelhouse liner.

Tighten
Tighten the bolts to 3.5 N·m (31 lb in).

3. Install the push-in retainers to the wheelhouse liner.