For 1990-2009 cars

### Removal Procedure

1. Pull back the drivers side wheelhouse liner to access the washer pump. Refer to Front Wheelhouse Liner Replacement in Body Front End.
2. Disconnect the electrical connector from the washer pump.
3. Disconnect the fluid hose from the washer pump, making sure to capture any spilling solvent.
4. Remove the washer pump from the washer solvent container by pulling firmly on the pump.

### Installation Procedure

1. Install the washer pump to the washer solvent container pressing into place until fully seated.
2. Connect the fluid hose from the washer pump.
3. Connect the electrical connector to the washer pump.
4. Fill the washer solvent container with new washer solvent.
5. Inspect the wiper/washer system for proper operation.
6. Pull back the drivers side wheelhouse liner. Refer to Front Wheelhouse Liner Replacement in Body Front End.