For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise vehicle on hoist.
2. Remove front transaxle mount through bolt.
3. Remove transaxle mount to transaxle bolts.
4. Remove transaxle mount from vehicle.

### Installation Procedure

1. Install transaxle mount to transaxle and tighten bolts.

Tighten
Tighten Front Transaxle Mount-to-Transaxle Bolts to: 90 N·m (66 lb ft)

2. Install transaxle mount through bolt and tighten.

Tighten
Tighten Front Transaxle Mount Through Bolt to: 55 N·m (41 lb ft)

3. Lower vehicle from hoist.