For 1990-2009 cars

#### Tools Required

J 36850 Transjel® Lubricant

1. Install the vehicle speed sensor O-ring (3) onto the input speed sensor (ISS) (2).

Apply J 36850 or an equivalent lubricant to the O-ring (3).

2. Install the ISS (2) into the converter housing.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the vehicle speed sensor bolt (1) into the converter housing.

Tighten
Tighten the bolt to 12 N·m (108 lb in).