For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Video System Schematics DEFINITION: With the rear video system on and a DVD playing, the radio off, the rear speakers do not play video audio through one side. With the rear video system on and no DVD playing, and the radio is on and RSA is off, radio audio plays from all rear speakers normally.
1 | Did you review the Video Entertainment System Description and Operation? | Go to Step 2 | Go to Video Entertainment System Description and Operation
2 |

1. Turn ON the ignition.
2. Turn on the wireless headphones.
3. Test the operation of the radio with the video entertainment system off. Radio audio plays through the vehicle speakers.
4. Turn off the radio.
5. Turn on the DVD player. Load a DVD in the DVD player. Start the DVD. Video audio plays through the vehicle speakers and the wireless headphones. The display plays video from the DVD player.
6. While the DVD is playing, turn the radio on. The rear speakers mute. The front speakers play radio audio. Video audio plays through the wireless headphones.

Does the system operate normally?

Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems

Go to Step 3

3 | Using the video remote control, test the balance and fade to the overhead and rear speakers. Does the system operate normally? | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems | Go to Step 4
4 | Are both left and right audio channels inoperative? | Go to Step 5 | Go to Step 6
5 | Test the DVD audio signal (-) circuit for an open. Test the VCP/DVD power enable signal circuit for an open or short to battery positive voltage. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 10 | Go to Step 7
6 | Test the appropriate DVD audio signal (+) circuit for an open or short to ground. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 10 | Go to Step 7
7 | Inspect for poor connections at the following harness connectors:

• | The AVI module

• | The radio connector

• | The digital video disc (DVD) player connector

Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems.

Did you find and correct the condition?

Go to Step 10

Go to Step 8

8 | Replace the digital video disc (DVD) player. Refer to Video Disc Player Replacement . Did you find and correct the condition? | Go to Step 10 | Go to Step 9
9 | Replace the radio. Refer to Radio Replacement . Did you complete the replacement? | Go to Step 10 | --
10 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3