For 1990-2009 cars

### Removal Procedure

1. Remove the center high-mounted stop lamp cover by pulling down at the edges.
2. Remove the bulbs, if required.
3. Disconnect the electrical connector from the center high-mounted stop lamp.
4. Remove the center high-mounted stop lamp by pulling down to release the retainer tabs.

### Installation Procedure

1. Position the center high-mounted stop lamp to the roof reinforcement.
2. Install the center high-mounted stop lamp by pressing into place until fully seated.
3. Connect the electrical connector to the high-mounted stop lamp.
4. Install new bulbs, if required.
5. Position the cover tabs to the slots.
6. Install the cover pressing into place until fully seated.