For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment lid applique. Refer to Rear Compartment Lid Applique Replacement .
2. Disconnect the latch cable from the lock cylinder.
3. Remove the retainer clip from the lock cylinder.
4. Remove the lock cylinder from the rear compartment lid.

### Installation Procedure

1. Position the lock cylinder to the rear compartment lid.
2. Install the retainer clip to the lock cylinder.
3. Connect the latch cable to the lock cylinder.
4. Install the rear compartment lid applique. Refer to Rear Compartment Lid Applique Replacement .