For 1990-2009 cars

### Removal Procedure

#### Left Side Shown, Right Side Similar

1. Remove the rear seat bolster. Refer to Rear Split Folding Seat Back Bolster Replacement in Seats.
2. Remove the shoulder belt from the comfort guide.
3. Remove the comfort guide retainer and remove the comfort guide.

### Installation Procedure

1. Install the comfort guide with the comfort guide retainer.
2. Install the comfort guide to the shoulder belt.
3. Install the rear seat bolster. Refer to Rear Split Folding Seat Back Bolster Replacement in Seats.
4. Test the shoulder belt assembly for the proper operation.