For 1990-2009 cars

### Removal Procedure

1. Remove the push-in retainers from the front of the front wheelhouse panel.
2. Remove the lower front fascia push-in retainers.
3. Remove the upper front fascia push-in retainers.
4. Disconnect the electrical connector from the fog lamp.
5. Disengage the fascia to the fender attaching tabs.
6. Slide the front fascia forward.
7. Remove the front bumper fascia from the vehicle.
8. If a new fascia is being installed, remove the following:

• | The front air deflector -- Refer to Front Bumper Fascia Air Deflector Replacement .

• | The front upper grille -- Refer to Front Bumper Upper Fascia Grille Replacement .

### Installation Procedure

1. If a new fascia is being installed, install the following:

• | The front air deflector -- Refer to Front Bumper Fascia Air Deflector Replacement .

• | The front upper grille -- Refer to Front Bumper Upper Fascia Grille Replacement .

2. Position the front bumper fascia to the vehicle.
3. Install the fascia ends over the shoulder bolts extending down from the front fender upper support bracket assembly, and push the fascia back.
4. Install the upper front fascia push-in retainers.
5. Install the lower front fascia push-in retainers.
6. Install the push-in retainers to the front of the front wheelhouse panel.
7. Connect the electrical connector to the fog lamp .