For 1990-2009 cars

1. Install the forward clutch support and lo roller clutch assembly (114) into the transmission case. Compress the parking pawl spring, and line up the parking pawl with the parking pawl gear.

Important: When installing the forward clutch support snap ring (112), the snap ring opening must be toward the bottom of the transmission case and facing the bottom pan.

2. Install the forward clutch support snap ring (112) into the transmission case with the ends pointing up. Use a screwdriver in order to set the snap ring into place.