For 1990-2009 cars

### Removal Procedure

1. Pull the control assembly boot down to disengage the boot from the knob.
2. Using a screwdriver, remove the control lever knob retainer.
3. Remove the control lever knob.
4. Pull up on the control boot until the indicator bezel disengages from the console.
5. Disconnect the indicator bezel electrical connector.
6. Remove the bezel and boot.
7. Disengage the control boot from the indicator bezel from the underside of the bezel.
8. Remove the boot.

### Installation Procedure

1. Install the control boot into the indicator bezel.
2. Install the bezel and boot over the shift lever and connect the indicator bezel electrical connector. Snap the bezel into the console opening.
3. Install the control lever knob and knob retainer.
4. Install the control assembly boot onto the knob so the O-ring in the top of the boot is seated in the groove on the bottom of the knob.