For 1990-2009 cars

#### Fastener Tightening Specifications

Description of Usage | Ref No.* | Qty | Size | Specification
--- | --- | --- | --- | ---
Metric | English
Bottom Pan to Case | 81 | 12 | M6x1.0x19.0 | 12 N·m | 106 lb in
Channel Plate to Case | 8 | 2 | M6x1.0x63.0 | 14 N·m | 124 lb in
Channel Plate to Case | 25 | 6 | M6x1.0x28.0 | 12 N·m | 106 lb in
Channel Plate to Driven Sprocket Support | 25 | 2 | M6x1.0x28.0 | 14 N·m | 124 lb in
Detent Spring Assembly to Channel Plate | 805 | 1 | M6x1.0x19.0 | 12 N·m | 106 lb in
Drive Sprocket Support Assembly to Case | 53 | 6 | M6x1.0x17.0 | 12 N·m | 106 lb in
Input Speed Sensor to Case | 15 | 1 | M6x1.0x15.0 | 12 N·m | 106 lb in
Intermediate 4th Servo Cover to Case | 25 | 3 | M6x1.0x28.0 | 12 N·m | 106 lb in
Line Pressure Plug to Case | 48 | 1 | 1/8-27NPTF | 12 N·m | 106 lb in
Lo/Reverse Servo Cover to Case | 25 | 3 | M6x1.0x28.0 | 12 N·m | 106 lb in
Oil Level Control Plug to Case | 65 | 1 | 1/8-27NPTF | 12 N·m | 106 lb in
Oil Tube Assembly To Case | 81 | 2 | M6x1.0x19.0 | 12 N·m | 106 lb in
Oil Tube Assembly to Forward Clutch | 81 | 1 | M6x1.0x19.0 | 12 N·m | 106 lb in
Oil Tube Assembly to Lo/Reverse Servo Cover | 81 | 1 | M6x1.0x19.0 | 12 N·m | 106 lb in
Output Shaft Speed Sensor to Case | 61 | 1 | M6x1.0x16.0 | 12 N·m | 106 lb in
Pump to Case | 9 | 1 | M6x1.0x103.0 | 12 N·m | 106 lb in
Pump to Channel Plate | 8 | 1 | M6x1.0x63.0 | 12 N·m | 106 lb in
Pump to Channel Plate | 12 | 6 | M6x1.0x90.0 | 12 N·m | 106 lb in
Side Cover to Case | 3 | 10 | M8x1.25x28.0 | 28 N·m | 22 lb ft
Side Cover to Case (Stud) | 4 | 1 | M8x1.25x28.0 | 28 N·m | 22 lb ft
Spacer to Driven Sprocket Support | 20 | 2 | M6x1.0x70.0 | 14 N·m | 124 lb in
TFP Switch Assembly to Case | 12 | 2 | M6x1.0x90.0 | 14 N·m | 124 lb in
TFP Switch to Channel Plate | 16 | 3 | M6x1.0x51.0 | 14 N·m | 124 lb in
TFP Switch to Channel Plate | 8 | 1 | M6x1.0x63.0 | 14 N·m | 124 lb in
Valve Body to Case | 9 | 2 | M6x1.0x103.0 | 14 N·m | 124 lb in
Valve Body to Case | 12 | 5 | M6x1.0x90.0 | 14 N·m | 124 lb in
Valve Body to Channel Plate | 16 | 5 | M6x1.0x51.0 | 14 N·m | 124 lb in
Wiring Harness Clip to Case | 15 | 1 | M6x1.0x15.0 | 12 N·m | 106 lb in
* Reference Number refers to the callout number on the disassembled view.

Application | Specification
--- | ---
Metric | English
Accessory Drive Belt Tensioner Assembly Bolts | 40 N·m | 30 lb ft
Air Pump-to-Bracket Bolts | 5.5 N·m | 49 lb in
Air Pump-to-Oil Pan Bolts | 25 N·m | 18 lb ft
Battery Cables-to-Battery | 17 N·m | 13 lb ft
Battery Feed Cable-to-Underhood Fuse Block Bolt | 16 N·m | 12 lb ft
Battery Hold Down Bracket Bolt | 20 N·m | 15 lb ft
Battery Tray Bolts | 15 N·m | 11 lb ft
Channel Plate-to-Case Bolts | 14 N·m | 10.5 lb ft
Channel Plate-to-Driven Sprocket Support Bolts | 14 N·m | 10.5 lb ft
Control Cable Mounting Bracket Bolts | 20 N·m | 15 lb ft
Control Valve Body Bolts | 12 N·m | 9 lb ft
Drive Sprocket Support Bolts | 12 N·m | 9 lb ft
Engine Cooling Fan Attachment Bolts | 4 N·m | 35 lb in
Engine-to-Transaxle Bolts | 65 N·m | 48 lb ft
Engine-to-Transaxle Bracket Bolts | 35 N·m | 26 lb ft
Exhaust Manifold Pipe Heat Shield Bolts | 8 N·m | 71 lb in
Exhaust Manifold Pipe-to-Exhaust Manifold Nuts | 30 N·m | 22 lb ft
Exhaust Manifold Pipe-to-Exhaust Pipe Bolts | 20 N·m | 15 lb ft
Flex Plate-to-Torque Convertor Bolts | 45 N·m | 33 lb ft
Front Transaxle Mount Through Bolt | 55 N·m | 41 lb ft
Generator Bolts | 40 N·m | 30 lb ft
Ground Wire Bolt | 25 N·m | 18 lb ft
Input Speed Sensor Bolt | 12 N·m | 9 lb ft
Lift Transaxle Mount Bracket-to-Transaxle Bolts | 90 N·m | 66 lb ft
Lower Control Arm-to-Steering Knuckle Nut and Bolt | 100 N·m | 75 lb ft
Oil Feed Pipe Assembly Bolts | 12 N·m | 9 lb ft
Oil Fan Bolts | 12 N·m | 9 lb ft
Oil Pump Bolts | 12 N·m | 9 lb ft
Output Speed Sensor Stud | 11 N·m | 8 lb ft
Power Steering Lines-to-Left Transaxle Mount Bracket | 10 N·m | 89 lb in
Servo Cover Bolts | 12 N·m | 9 lb ft
Side Cover-to-Transaxle Case Bolts | 20 N·m | 15 lb ft
Spacer Plate Support Bolts | 14 N·m | 10.5 lb ft
Speed Sensor Stud | 12 N·m | 9 lb ft
Splash Shield Fasteners | 5 N·m | 44 lb in
Stabilizer Bar Link-to-Strut Assembly | 65 N·m | 48 lb ft
Starter Assembly Bolts | 40 N·m | 30 lb ft
Steering Gear Heat Shield | 4 N·m | 35 lb in
Steering Gear-to-Frame Assembly Bolts | 45 N·m + 45-60° | 33 lb ft + 45-60°
Suspension Support-to-Frame Bolts | 90 N·m + 45-60° | 66 lb ft + 45-60°
Transaxle Control Module (TCM) Cover Nuts | 3 N·m | 27 lb in
Transaxle Cooler Line Fittings | 25 N·m | 18 lb ft
Transaxle Fluid Level Plug | 12 N·m | 9 lb ft
Transaxle Mount (Left)-to-Engine Compartment Rail Bolts | 20 N·m | 15 lb ft
Transaxle Mount (Left)-to-Transaxle Mount Bracket Bolts | 55 N·m | 41 lb ft
Transaxle Mount (Rear) Through Bolts | 90 N·m | 66 lb ft
Transaxle Mount (Rear)-to-Frame Assembly Bolts | 60 N·m | 44 lb ft
Transaxle Mounts (Front and Rear)-to-Transaxle Bolts | 90 N·m | 66 lb ft
Transaxle Oil Cooler Line Assembly Nut | 8 N·m | 71 lb in
Transaxle Range Switch Bolts | 20 N·m | 15 lb ft
Transaxle Range Switch Lever Nut | 35 N·m | 26 lb ft
Transaxle Support Fixture (J43707) Bolts | 11 N·m | 8 lb ft
Underhood Fuse Block Case Bolt | 9 N·m | 80 lb in
Wheel Bolts (Final Torque) | 125 N·m | 92 lb ft
Wheel Bolts (Initial Torque) | 63 N·m | 46 lb ft
Wiring Harness Attachment Fasteners | 20 N·m | 15 lb ft
Wiring Harness Retainer Bolt | 12 N·m | 9 lb ft