For 1990-2009 cars

#### Tools Required

J 43773 Valve Spring Compressor

1. Install the shift solenoid screen (1).
2. Measure the screen installation depth at dimension A.

Specification
The screen installed depth is 0.50-1.0 mm (0.020-0.039 in) below the shift valve body surface as shown.

3. Install the control main valve (1) and the control main spring (2).
4. Compress the spring with J 43773 (2).
5. Install the retaining clip (1).
6. Make sure the retaining clip is below the valve body surface.
7. Install shift solenoid D shift valve (1), spring (2), and plug (3).
8. Compress the spring with J 43773 (2).

Install the retaining clip (1).

9. Make sure the retaining clip is below the valve body surface.
10. Install shift solenoid E shift valve (1), the spring (2), and plug (3).
11. Compress the spring with J 43773 (2).
12. Install the retaining clip (1).
13. Make sure the retaining clip is below the valve body surface.
14. Install shift solenoid C shift valve (1) and spring (2).
15. Compress the spring with J 43773 (2).
16. Install the retaining clip (1).
17. Make sure the retaining clip is below the valve body surface.