For 1990-2009 cars

### Removal Procedure

Caution: Keep fingers away from rear brake shoe springs to prevent fingers from being pinched between spring and shoe web or spring and backing plate.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the brake drum. Refer to Brake Drum Replacement .

Notice: Do not over stretch the adjuster spring. Damage can occur if the spring is over stretched.

3. Disengage the adjuster spring hook end from the tab on the adjuster actuator (1).
4. Remove the straight end of the adjuster spring from the brake shoe.
5. Remove the adjuster actuator from the brake shoe.
6. Remove the return spring (7) from the brake shoes.
7. Remove the park brake cable (6) from the park brake actuator lever (5).
8. Remove the brake shoe hold-down springs and retainers (4) from the brake shoes.
9. Remove the adjuster from the brake shoes and the park brake actuator lever.
10. Remove the horseshoe clip retaining the park brake actuator lever to the brake shoe.
11. Remove the park brake actuator lever and wave washer from the brake shoe.
12. Clean all of the drum brake system components with denatured alcohol.
13. Inspect all of the drum brake system components. Refer to Drum Brake Hardware Inspection .
14. Replace drum brake system components as necessary. Refer to Drum Brake Hardware Replacement .
15. Inspect the wheel cylinder for the following conditions:

• | Brake fluid leakage

• | Worn or damaged dust boots

16. Replace damaged or leaking wheel cylinders as necessary. Refer to Wheel Cylinder Replacement .

### Installation Procedure

1. Apply GM P/N 1052196 brake lubricant (or equivalent) to the following areas:

• | The brake shoe contact points on the backing plate

• | The adjuster screw threads

• | The inside diameter of the adjuster socket

2. Install the park brake actuator lever and wave washer to the brake shoe.
3. Install the horseshoe clip to the park brake actuator lever pivot pin.
4. Install the brake shoes to the brake backing plate.
5. Install the brake shoe hold-down pins, springs and retainers (4) to the brake shoes.
6. Install the park brake cable (6) to the park brake actuator lever.

Important: Ensure that the adjuster (2) engages the brake shoe (4) and the park brake actuator (3) properly.

7. Install the adjuster screw to the brake shoe and the park brake actuator.
8. Apply GM P/N 1052196 brake lubricant (or equivalent) to the adjuster actuator/brake shoe interface.
9. Install the adjuster actuator (1) to the brake shoe.

Notice: Do not over stretch the adjuster spring. Damage can occur if the spring is over stretched.

10. Install the straight end of the adjuster spring (3) to the brake shoe.
11. Install the adjuster spring hook end to the tab on the adjuster actuator (1).
12. Install the return spring (7) to the brake shoes.

Important: Ensure that the adjuster operates properly.

13. Move the park brake actuator lever (5) in order to spread the brake shoes apart. The adjuster actuator lever should move downward, then upward as the park brake actuator lever is released, forcing the adjuster wheel to rotate.

If the adjuster does not operate properly, remove then reinstall the adjuster.

14. Adjust the brake shoes. Refer to Drum Brake Adjustment .
15. Adjust the park brake cable. Refer to Park Brake Adjustment in Park Brake.
16. Install the brake drum. Refer to Brake Drum Replacement .
17. Lower the vehicle.