For 1990-2009 cars

## Fastener Tightening Specifications 4WD

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 20 N·m | 15 lb ft
Clutch Housing Bolts | 45 N·m | 33 lb ft
Countershaft Center Bearing Plate Bolts | 10 N·m | 89 lb in
Gearshaft Lever Case Bolts | 17 N·m | 13 lb ft
Input Shaft Bearing Retainer Bolts | 23 N·m | 17 lb ft
Lever Locating Bolts | 20 N·m | 15 lb ft
Locating Spring Bolts | 28 N·m | 21 lb ft
Rear Case Bolts | 23 N·m | 17 lb ft
Reverse Gearshift Limit Bolt | 35 N·m | 26 lb ft
Reverse Idler Shaft Bolt | 22 N·m | 16 lb ft
Select Return Spring Bolts | 23 N·m | 17 lb ft
Transfer Case-to-Transmission Bolts | 28 N·m | 21 lb ft
Upper-to-Lower Case Retaining Bolts | 23 N·m | 17 lb ft

## Fastener Tightening Specifications 2WD

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 20 N·m | 15 lb ft
Clutch Housing Bolts | 45 N·m | 33 lb ft
Countershaft Center Bearing Plate Bolts | 6 N·m | 53 lb in
Extension Case Bolts | 23 N·m | 17 lb ft
Gearshift Lever Case Bolts | 17 N·m | 13 lb ft
Input Shaft Bearing Retainer Bolts | 23 N·m | 17 lb ft
Lever Locating Bolts | 20 N·m | 15 lb ft
Locating Spring Bolts | 28 N·m | 21 lb ft
Reverse Gearshift Limit Bolt | 35 N·m | 26 lb ft
Reverse Idler Shaft Bolt | 22 N·m | 16 lb ft
Select Return Spring Bolts | 23 N·m | 17 lb ft
Speedometer Driven Gear Case Retaining Bolt | 12 N·m | 106 lb in
Upper-to-Lower Case Retaining Bolts | 23 N·m | 17 lb ft