For 1990-2009 cars

### Removal Procedure

1. Reach down into the outer corner of the rear seat cushion to expose the bolster retaining tab.
2. Bend the tab upward.
3. Remove the seat bolster:

3.1. | Remove the lower end of the bolster.

3.2. | Push upward to remove the top end of the bolster.

### Installation Procedure

Important: Verify that the rear seat shoulder belt is not caught behind bolster when installing the bolster.

1. Position the seat bolster onto the upper bolster attachment.
2. Push down on the bolster to engage the upper attachment and install over the retaining tab.
3. Bend the lower retaining tab over the bolster wire frame at the seat cushion location.