For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Check Link to Body Bolt | 10 N·m | 89 lb in
Door and Reinforcement Plate to Hinge Nuts | 30 N·m | 22 lb ft
Door Check Link to Body Bolt | 10 N·m | 89 lb in
Door Check Link to Hinge Pillar Bolt | 10 N·m | 89 lb in
Door Hinge to Hinge Pillar Bolts | 30 N·m | 22 lb ft
Door Striker to Body Bolts | 20 N·m | 15 lb ft
Door Trim Panel Fasteners | 1.5 N·m | 13 lb in
Door Trim Panel Lower Fasteners | 1.5 N·m | 13 lb in
Front Window Regulator Bolts | 10 N·m | 89 lb in
Hinge Fasteners | 30 N·m | 22 lb ft
Latch to Door Bolts | 10 N·m | 89 lb in
Mirror Attachment Nuts | 10 N·m | 89 lb in
Mirror Motor to Mirror Housing Screws | 3 N·m | 27 lb in
Outer Belt Seal Fasteners | 2 N·m | 18 lb in
Outer Door Panel Fasteners (Use Threadlocker) | 6 N·m | 53 lb in
Rear Window Regulator Bolts | 10 N·m | 89 lb in
Weatherstrip Guide Bolts | 10 N·m | 89 lb in
Window Guide Bolt | 10 N·m | 89 lb in
Window Run Channel Fastener | 10 N·m | 89 lb in