For 1990-2009 cars

## Rear License Plate Lamp Replacement Wagon

### Removal Procedure

1. Remove the license lamp screws on each side.
2. Pull the lamp down.
3. Remove the bulb(s), if required.

### Installation Procedure

1. Install the bulb(s), if required.
2. Install the license lamp by positioning the lens into opening.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the license lamp screws on each side.

Tighten
Tighten the screws to 2 N·m (18 lb in).

## Rear License Plate Lamp Replacement Sedan

### Removal Procedure

1. Remove the license lamp screws on each side.
2. Pull the lamp down.

### Installation Procedure

1. Install the license lamp by positioning the lens into the opening.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the license lamp screws on each side.

Tighten
Tighten the screws to 2 N·m (18 lb in).