For 1990-2009 cars
Auto Learn Timer: The scan tool displays the seconds used by the body control module (BCM) to learn valid code from the Passlock™ sensor. The learn procedure consists of 3 consecutive periods.
Battery Voltage: The scan tool displays the battery system voltage.
Content Theft Lamp: The scan tool displays the state of the SECURITY lamp. The scan tool displays ON when activated by an unauthorized entry.
Content Theft State: The scan tool displays the state of the content theft feature. The scan tool displays ON when activated by an unauthorized entry.
Door Handle Switch: The scan tool displays the position of the door handle. The scan tool displays ACTIVE when a door handle is raised and INACTIVE with all doors closed and the door handles at rest.
Door Key Switch: The scan tool displays the state of the door key switch. The scan tool displays ACTIVE when the switch is activated in either door key cylinder.
Drivers Door Jamb Switch: The scan tool displays the position of the drivers door. The scan tool displays ACTIVE when the drivers door is open.
Ignition 1: The scan tool displays the state of the ignition switch. The scan tool displays ACTIVE when the ignition switch is in the RUN or CRANK position.
Ignition 3: The scan tool displays the state of the ignition switch. The scan tool displays ACTIVE when the ignition switch is in the RUN position.
Manufacture Enable Counter (MEC): The scan tool displays the actual value for the MEC in the BCM. This information is for the assembly plant only.
Module Part Number: The scan tool displays the part number assigned to the BCM that is currently in the vehicle.
Passlock™ Code: The scan tool displays the validity of the Passlock™ code received by the BCM. The scan tool displays OPEN, SHORTED, TAMPER and a valid code as a numeric value (1-10).
Passlock™ Data Voltage: The scan tool displays the voltage code from the Passlock sensor to the BCM. A valid Passlock sensor voltage of 5-volts will be displayed on the scan tool when the ignition cylinder is turned to the on position. Once the ignition cylinder has been rotated to the crank position the Passlock voltage will drop from 5 to 0.86-4.28 volts depending on which of the 10 possible Passlock sensors the vehicle is equipped with. The BCM then determines if the voltage received is a valid or invalid code. The scan tool will continue to display the Passlock voltage code (0.86-4.28 volts) received by the BCM when the ignition cylinder returns to the on/run position.
Passlock™ State: The scan tool displays the state of the Passlock™ system.
Security Calibration Number: The scan tool displays the security calibration part number in the BCM.
Security Lamp State: The scan tool displays the state of the SECURITY lamp. The scan tool displays ON, OFF or FLASHING.
Security Suffix: The scan tool displays the security identification number in the BCM.
Tamper Timer: The scan tool displays the time remaining when in the tamper mode. The timer starts when the ignition switch is turned to the RUN position and the BCM receives a Passlock™ data voltage different from the last learned voltage. The timer has a delay of 10 minutes and will stay active even if the ignition switch is cycled from the RUN to the OFF position.
VCM/PCM Fail Enable: The scan tool displays the state of the VCM/PCM fail enable mode. The scan tool displays YES when the Passlock™ system transitions from the Monitor Passlock™ Data state to the VCM/PCM Fail Enable state.
VCM/PCM Fuel Continue: The scan tool displays the state of the VCM/PCM fuel continue mode. The scan tool displays YES when the Passlock™ system verifies a valid password to the BCM.
VCM/PCM Learn Timer: The scan tool displays the state of the VCM/PCM learn timer. The scan tool displays INACTIVE when the BCM is not in a learn mode.
VTD Fuel Disable: The scan tool displays the state of the VTD fuel disable mode. The scan tool displays INACTIVE when the Passlock™ system verifies a valid password.
VTD Fuel Disable Until Ignition Off: The scan tool displays the state of the VTD fuel disable until Ignition off mode. The scan tool displays NO when the Passlock™ system verifies a valid password.
VTD Password Learn Mode: The scan tool displays the state of the VTD password learn mode. The scan tool displays INACTIVE when the Passlock™ system is not in a learn mode.