For 1990-2009 cars

### Removal Procedure

1. Open the fuel filler door.
2. Remove the bolts holding the fuel filler door to the quarter panel.
3. Remove the fuel filler door from the quarter panel.

### Installation Procedure

1. Position the fuel filler door to the quarter panel.
2. Loosely install the bolts holding the fuel filler door to the quarter panel.

Align the fuel filler door to the quarter panel.

Notice: Refer to Fastener Notice in the Preface section.

3. Tighten the fuel filler door bolts.

Tighten
Tighten the bolts to 1 N·m (9 lb in).