For 1990-2009 cars

### Removal Procedure

1. Open the liftgate.
2. Flip up the side wings and lift the rear load floor from the vehicle.
3. Remove the child restraint bracket fasteners and remove the bracket.
4. Lower the rear seat backs.
5. Remove the front load floor retainers and remove the load floor.

### Installation Procedure

1. Position the load floor into the vehicle.
2. Raise the rear seat backs.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the child restraint bracket with the fasteners.

Tighten
Tighten the fasteners to 20 N·m (15 lb ft).

4. Install the rear load floor.
5. Close the liftgate.