For 1990-2009 cars

#### Tools Required

• | J 36190 Universal Drive Handle

• | J 36798 Shift Rail Bushing Staking Tool

1. Install the input shaft bearing using a brass drift on the outer race of the bearing.
2. Install the countershaft front bearing race using a suitable bearing installer.

Important: When installing the front shift shaft bushing into the clutch housing, ensure the bushing split line is not aligned with the hydrolock in the clutch housing.

3. Using the J 36798 (2) with the bushing side against the bushing, and the J 36190 (1), install the shift shaft bushing in the clutch housing.
4. Using the J 36798 with the stake side of the J 36798-2 against the bushing, and the J 36190 , stake the bushing in place.
5. Inspect the bushing for proper installation by installing the main shift rail in the bushing. The shift rail should slide easily in the bushing.
6. Install the vent, if removed. The vent taps into the clutch housing.