For 1990-2009 cars

### Removal Procedure

1. Remove the lift gate trim panel. Refer to Liftgate Trim Panel Replacement .
2. Disconnect the electrical connector from the lock assembly.
3. Remove the lift gate lock assembly nuts.
4. Disconnect the latch cable from the lock cylinder.
5. Remove the lock cylinder.

### Installation Procedure

1. Connect the latch cable to the latch assembly.
2. Position the lock cylinder to the lift gate.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the lock cylinder nuts.

Tighten
Tighten the nuts to 3 N·m (27 lb in).

4. Connect the electrical connector to the lock assembly.
5. Install the lift gate trim panel. Refer to Liftgate Trim Panel Replacement .