For 1990-2009 cars

## Power Steering Pump Pulley Replacement L81

### Removal Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement in Engine Controls-3.0L (L81).
2. Remove the power steering pump pulley bolts.
3. Remove the accessory drive belt.
4. Remove the pulley from the power steering pump.

### Installation Procedure

1. Align the power steering pulley to the pump hub while loosely installing the pulley bolts.
2. Install the accessory drive belt.

Notice: Refer to Fastener Notice in the Preface section.

3. Tighten the power steering pulley to pump bolts.

Tighten
Tighten the bolts to 20 N·m (15 lb ft).

4. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement in Engine Controls-3.0L (L81).