For 1990-2009 cars

1. Remove the following components from the rear adapter case (2):

• | The VSS bolt

• | The VSS (1)

2. Remove the following rear adapter case components from the transmission case:

• | The bolts

• | The case

• | The gasket

3. Remove the cooler lines (1) and remove the fittings (2).
4. Remove the following components from the rear output shaft:

• | The VSS snap ring (2)

• | The VSS rotor (1)

• | The key-way

• | The rear cover plate and screws (3)